use Armakleen 2002 in the wash sections.
     temp. in the wash is 160f. @ 50 psi, speed 2 fpm.

Questions:
     Anyone else have this problem?
     What have you done to correct it?
     Is there a parts marking spec?

Thanks in advance for your help.

Phil Belliveau
Sippican, Inc
508-748-1160 x379 
     
each incident.

    Each board is cleaned 3 times.
1st time after smt reflow.
2nd time after wave solder.
3rd time before shipping.

     We have a Westkleen in line system.
     We0000 Armakleen 2002 in the wash sections.
     temp. in the wash is 160f. @ 50 psi, speed 2 fpm.

Questions:
     Anyone else have this problem?
     What have you done to correct it?
     Is there a parts marking spec?

Thanks in advance for your help.

Phil Belliveau
Sippican, Inc
508-748-1160 x379